Legion Brothers   Obsessed with innovations
Technical specification
Computerized Heat Transfer in Lagged pipe Apparatus
Product code: HMTC04     Category: Heat & Mass Transfer
Description
The apparatus consists of a metal pipe with two layers of insulation. An electric heating coil wound on a silica rod is placed at the center. The ends are thickly insulated to prevent heat loss so that, heat flow only in a radial direction. Three thermocouples each are placed at different radii to measure the temperature distribution within the cylinder.
Experiments that can be performed
Determine the thermal conductivity of the lagging (insulating) material
Plot the radial temperature distribution through the lagging
Features
Extensive range of Experiments
Comprehensive teaching manual
Three-year warranty
Aesthetically designed and finished Rig
High Quality instrumentation
Scope of supply
Supply of the rig as specified, with data acquisition and software where listed
Installation and commissioning at site
Training for laboratory staff
Annual maintenance contract (AMC), if applicable
Delivery period and payment terms are given in the quotation.
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