Legion Brothers   Obsessed with innovations
Technical specification
Computerized Shell and Tube Heat exchanger
Product code: HMTC09     Category: Heat & Mass Transfer
Description
This equipment allows students to fully investigate the performance and characteristic of a shell and multi tube heat exchanger. It consists of 12 tubes of 12mm outside diameter and the effective length of the tube is 1000mm with two tube pass. The shell is made of stainless steel having inside diameter of 150mm with 6 segmental baffles. The water flow rate is measured using a rotameter. Thermocouples are provided for measuring the inlet and outlet temperature hot and cold fluids.
Experiments that can be performed
Determine the overall heat transfer coefficient
Determine the effectiveness of the heat exchanger
Features
Extensive range of Experiments
Comprehensive teaching manual
Three-year warranty
Aesthetically designed and finished Rig
High Quality instrumentation
Scope of supply
Supply of the rig as specified, with data acquisition and software where listed
Installation and commissioning at site
Training for laboratory staff
Annual maintenance contract (AMC), if applicable
Delivery period and payment terms are given in the quotation.
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