Legion Brothers   Obsessed with innovations
Technical specification
Manifold Gas Injection Kit with Open ECU and EGR
Product code: R&DU01     Category: Research Equipment
Description
A manifold gas injection kit suitable for any single-cylinder engine, with gas injected into the intake manifold.
The ECU of a standard aftermarket gas kit cannot be used on a research engine: its injection start angle and duration come from preprogrammed maps, while finding the optimal map values is part of the research itself. This kit therefore comes with an open-loop electronic control unit (Open ECU) on which the user sets the injection start angle and injection duration. The ECU is designed, programmed and tested by Legion Brothers and is supplied only to research users.
Features
Crankshaft position sensor (Measures crankshaft position)
Camshaft position sensor - (Measures camshaft position)
MAF Sensor - (Measures mass air flow)
Map sensor - (Measures manifold temperature and pressure)
Engine Control Unit - (To Measure sensors and control series of actuators on an internal combustion engine and ensure excellent engine performance)
Gas injector – (For fuel injection)
EGR Valve - (Re-circulates controlled flow of exhaust gas into the intake)
Can + K line - (For calibration and Troubleshoot)
Scope of supply
Supply of the rig as specified, with data acquisition and software where listed
Installation and commissioning at site
Training for laboratory staff
Annual maintenance contract (AMC), if applicable
Delivery period and payment terms are given in the quotation.
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