Legion Brothers   Obsessed with innovations
Technical specification
CRDI Kit – Open ECU with EGR
Product code: R&DU04     Category: Open ECU
Description
An Open ECU kit for common-rail diesel (CRDI) engines, with EGR.
The user sets the idle speed (with closed-loop idle control), the start angles of pilot and main injection, the injection duration in crank-angle degrees, open-loop rail pressure from 200 to 1100 bar, and EGR flow. Calibration charts for injection quantity at various rail pressures are supplied, and CAN and K-line access is provided for calibration and troubleshooting.
Features
Crankshaft position sensor (Measures crankshaft position)
Camshaft position sensor - (Measures camshaft position)
MAF Sensor - (Measures mass air flow)
Rail pressure sensor - (Measures common rail pressure)
T Map sensor - (Measures manifold temperature and pressure)
Engine Control Unit - (To Measure sensors and control series of actuators on an internal combustion engine and ensure excellent engine performance)
Diesel solenoid injector – (For fuel injection)
EGR Valve - (Re-circulates controlled flow of exhaust gas into the intake)
Can + K line - (For calibration and Troubleshoot)
Scope of supply
Supply of the rig as specified, with data acquisition and software where listed
Installation and commissioning at site
Training for laboratory staff
Annual maintenance contract (AMC), if applicable
Delivery period and payment terms are given in the quotation.
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