Legion Brothers   Obsessed with innovations
Technical specification
GDI Kit – Open ECU with EGR
Product code: R&DU13     Category: Open ECU
Description
An Open ECU kit for gasoline direct injection (GDI) engines.
The user sets the idle speed (with closed-loop idle control), the start of injection for homogeneous operation, the end of injection for stratified operation, the spark timing, and open-loop rail pressure from 10 to 110 bar; injection duration is calculated by the ECU. Calibration charts for injection quantity are supplied, and CAN and K-line access is provided for calibration and troubleshooting.
Features
Crankshaft position sensor (Measures crankshaft position)
Camshaft position sensor - (Measures camshaft position)
MAF Sensor - (Measures mass air flow)
Rail pressure sensor - (Measures common rail pressure)
T Map sensor - (Measures manifold temperature and pressure)
Engine Control Unit - (To Measure sensors and control series of actuators on an internal combustion engine and ensure excellent engine performance)
Petrol solenoid injector – (For fuel injection)
EGR Valve - (Re-circulates controlled flow of exhaust gas into the intake)
Can + K line - (For calibration and Troubleshoot)
Scope of supply
Supply of the rig as specified, with data acquisition and software where listed
Installation and commissioning at site
Training for laboratory staff
Annual maintenance contract (AMC), if applicable
Delivery period and payment terms are given in the quotation.
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