Legion Brothers   Obsessed with innovations
Technical specification
Computerized Heat Pipe Demonstrator
Product code: HMTC15     Category: Heat & Mass Transfer
Description
The apparatus is designed to reveal clearly the conducting material. It consists of three identical cylindrical pipes, one end of the pipes is heated electrically and the other end is cooled by water. Thermocouples are embedded along the lengths to measure the temperature distribution. Heat input is measured by digital voltmeter and ammeter. The temperatures at various points are measured by thermocouples and indicated in a digital temperature indicator.
Experiments that can be performed
Study the performance of a heat pipe and the temperature distribution along its length
Features
Extensive range of Experiments
Comprehensive teaching manual
Three-year warranty
Aesthetically designed and finished Rig
High Quality instrumentation
Scope of supply
Supply of the rig as specified, with data acquisition and software where listed
Installation and commissioning at site
Training for laboratory staff
Annual maintenance contract (AMC), if applicable
Delivery period and payment terms are given in the quotation.
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